	Xvisor on Xilinx ZynqMP ZCU102 using SD Booting

This section of readme explains how to build & run Xvisor on ZynqMP
ZCU102 board using SD booting.

By default, Xvisor for ZynqMP supports Virt-v8 guest so we will show how
to boot Linux using Basic Firmware on Virt-v8 guest.

The ZynqMP ZCU102 usually comes with and SD card containig the FABL and
u-boot to boot the ARM processor. We will add 3 more images to the boot
partition of SD card:
 1) U-Boot compatible Xvisor binary (uvmm.bin)
 2) DTB for Xvisor (zynqmp-zcu102.dtb)
 3) U-Boot compatible Xvisro disk containing guest binaries (udisk.img)

Following are steps to create these images and boot Xvisor on ZynqMP:

  [1. Build environment]
  # export CROSS_COMPILE=aarch64-linux-gnu-

  [2. GoTo Xvisor source directory]
  # cd <xvisor_source_directory>

  [3. Configure Xvisor with Generic-v8 default settings]
  # make ARCH=arm generic-v8-defconfig

  [4. Build Xvisor and DTBs]
  # make

  [5. Make U-Boot compatible uvmm.bin for use with bootm command]
  # mkimage -A arm64 -O linux -T kernel -C none -a 0x00080000 -e 0x00080000 -n Xvisor -d build/vmm.bin build/uvmm.bin

  [6. Build Basic Firmware]
  # make -C tests/arm64/virt-v8/basic

  [7. GoTo Linux source directory]
  # cd <linux_source_directory>

  [8. Configure Linux in build directory]
  # cp arch/arm64/configs/defconfig arch/arm64/configs/tmp-virt-v8_defconfig
  # <xvisor_source_directory>/tests/common/scripts/update-linux-defconfig.sh -p arch/arm64/configs/tmp-virt-v8_defconfig -f <xvisor_source_directory>/tests/arm64/virt-v8/linux/linux_extra.config
  # make O=<linux_build_directory> ARCH=arm64 tmp-virt-v8_defconfig

  [9. Build Linux in build directory]
  # make O=<linux_build_directory> ARCH=arm64 Image dtbs

  [10. Create BusyBox RAMDISK to be used as RootFS for Linux kernel]
  (Note: For subsequent steps, we will assume that your RAMDISK is located at <busybox_rootfs_directory>/rootfs.img)
  (Note: Please refer tests/common/busybox/README.md for creating rootfs.img using BusyBox)

  [11. GoTo Xvisor source directory]
  # cd <xvisor_source_directory>

  [12. Create disk image for Xvisor with Guest Linux and Guest Basic Firmware]
  # mkdir -p ./build/disk/tmp
  # mkdir -p ./build/disk/system
  # cp -f ./docs/banner/roman.txt ./build/disk/system/banner.txt
  # cp -f ./docs/logo/xvisor_logo_name.ppm ./build/disk/system/logo.ppm
  # mkdir -p ./build/disk/images/arm64/virt-v8
  # dtc -q -I dts -O dtb -o ./build/disk/images/arm64/virt-v8-guest.dtb ./tests/arm64/virt-v8/virt-v8-guest.dts
  # cp -f ./build/tests/arm64/virt-v8/basic/firmware.bin ./build/disk/images/arm64/virt-v8/firmware.bin
  # cp -f ./tests/arm64/virt-v8/linux/nor_flash.list ./build/disk/images/arm64/virt-v8/nor_flash.list
  # cp -f ./tests/arm64/virt-v8/linux/cmdlist ./build/disk/images/arm64/virt-v8/cmdlist
  # cp -f ./tests/arm64/virt-v8/xscript/one_guest_virt-v8.xscript ./build/disk/boot.xscript
  # cp -f <linux_build_directory>/arch/arm64/boot/Image ./build/disk/images/arm64/virt-v8/Image
  # dtc -q -I dts -O dtb -o ./build/disk/images/arm64/virt-v8/virt-v8.dtb ./tests/arm64/virt-v8/linux/virt-v8.dts
  # cp -f <busybox_rootfs_directory>/rootfs.img ./build/disk/images/arm64/virt-v8/rootfs.img
  # genext2fs -B 1024 -b 32768 -d ./build/disk ./build/disk.img
  OR
  [12. Create disk image for Xvisor with only Guest Basic Firmware]
  # mkdir -p ./build/disk/tmp
  # mkdir -p ./build/disk/system
  # cp -f ./docs/banner/roman.txt ./build/disk/system/banner.txt
  # cp -f ./docs/logo/xvisor_logo_name.ppm ./build/disk/system/logo.ppm
  # mkdir -p ./build/disk/images/arm64/virt-v8
  # dtc -q -I dts -O dtb -o ./build/disk/images/arm64/virt-v8-guest.dtb ./tests/arm64/virt-v8/virt-v8-guest.dts
  # cp -f ./build/tests/arm64/virt-v8/basic/firmware.bin ./build/disk/images/arm64/virt-v8/firmware.bin
  # cp -f ./tests/arm64/virt-v8/linux/nor_flash.list ./build/disk/images/arm64/virt-v8/nor_flash.list
  # cp -f ./tests/arm64/virt-v8/xscript/one_guest_virt-v8.xscript ./build/disk/boot.xscript
  # genext2fs -B 1024 -b 32768 -d ./build/disk ./build/disk.img

  [13. Make U-boot compatible udisk.img for use with bootm command]
  # mkimage -A arm64 -O linux -T ramdisk -a 0x00000000 -n "Xvisor Ramdisk" -d build/disk.img build/udisk.img

  [14. Unplug bootable SD card from the ZynqMP ZCU102 board and plug it on your development machine]

  [15. Mount data partition (or partition 2) of SD card on your development machine]

  [16. Copy uvmm.bin, DTB, and udisk.img to data partition of SD card]
  # cp -f build/uvmm.bin <path_to_mounted_data_partition_of_sd_card>
  # cp -f build/arch/arm/board/generic/dts/xilinx/zynqmp-zcu102.dtb <path_to_mounted_data_partition_of_sd_card>
  # cp -f build/udisk.img <path_to_mounted_data_partition_of_sd_card>

  [17. Unmount data partition (or partition 0) of SD card from your development machine]

  [18. Unplug SD card from your development machine and plug it back on ZynqMP ZCU102 board]

  [19. Connect to serial port of ZynqMP ZCU102 board using Putty or Minicom]

  [20. Power-up or Reset ZynqMP ZCU102 board and press any key when U-Boot shows auto-boot count down]

  [21. Copy Xvisor from SD card to SDRAM]
  U-Boot> fatload mmc 0 0x200000 uvmm.bin

  [22. Copy the Xvisor DTB from SD card to SDRAM]
  U-Boot> fatload mmc 0 0x800000 zynqmp-zcu102.dtb

  [23. Copy disk image from SD card to SDRAM]
  U-Boot> fatload mmc 0 0x2000000 udisk.img

  [24. Jump into Xvisor after disabling MMU, interrupts, etc]
  U-Boot> bootm 0x200000 0x2000000 0x800000

  [25. Kick Guest0 for starting Basic Firmware]
  XVisor# guest kick guest0

  [26. Bind to virtual UART]
  XVisor# vserial bind guest0/uart0

  [27. Try few commands of Basic firmware or goto next step]
  [guest0/uart0] basic# hi
  [guest0/uart0] basic# hello
  [guest0/uart0] basic# help

  [28. Copy linux from NOR flash to RAM and start linux booting from RAM]
  [guest0/uart0] basic# autoexec
  (Note: "autoexec" is a short-cut command)
  (Note: The <xvisor_source_directory>/tests/arm64/virt-v8/linux/cmdlist
   file which we have added to guest NOR flash contains set of commands for booting
   linux from NOR flash)

  [29. Wait for Linux prompt to come-up and then try out some commands]
  [guest0/uart0] / # ls

  [30. Enter character seqence 'ESCAPE+x+q" return to Xvisor prompt]
  [guest0/uart0] / #

  (Note: replace all <> brackets based on your workspace)
  (Note: for more info on your desired ARM host refer docs/arm/)
  (Note: you are free to change the ordering of above steps based
   on your workspace)
